
Installation/Update KNX IP BAOS 777

DE

Zip Datei entpacken (falls noch nicht geschehen) und die .wzpkg Datei im Webinterface des Geräts 
(erreichbar über Browser durch Eingabe der im Gerätedisplay abzulesenden IP-Adresse), 
über das Feld Device update auf dem Device Reiter, hochladen. 
Während des Updates das Gerät nicht vom KNX Bus oder von der Spannungsversorung bzw. LAN trennen.
Für nähere Informationen konsultieren Sie bitte das Manual des KNX IP BAOS 777.

++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++

EN

Unzip the zip package (in case you haven't already) and upload the .wzpkg file to the device. 
You can do this via the web application found on the KNX IP BAOS 777 by entering the IP address 
of the device displayed on the front LCD into the address bar of your favourite web browser. 
Enter your username and password, navigate to the bottom of the Device tab and click on the upload square. 
Do not disconnect the device from the KNX bus or from the power supply or LAN during the update.
This information is described in detail in the User Manual of the KNX IP BAOS 777.



Contact

Web:   www.weinzierl.de
Email: support@weinzierl.de

Weinzierl Engineering GmbH
Achatz 3-4
DE-84508 Burgkirchen / Alz
Germany
